**GO-DEVIL® MANUFACTURING CO. OF LOUISIANA, L.L.C.**

18649 Womack Road \* Baton Rouge, LA 70817

(225) 752-0167 \* Fax (225) 752-0175

www.godevil.com

**SERVICE BULLETIN**

**ALL FNR ENGINES WITH BLUE LOCTITE**

**NO. SDFNR1**

**DATE: 5/5/20**

**RE:** All FNR Engines

**CONDITION FOUND:**  Center bolt loosened on crankshaft with Blue Loctite.

**CORRECTIVE ACTION:** Use Red Loctite #263 on center bolt. Coat the full length of threads and torque to 78 foot-pounds. Pre-clean with brake cleaner and then clean again with denatured alcohol before applying Red Loctite.